****************************************************************

  las2shp:

  converts LIDAR from LAS/LAZ/ASCII to ESRI's Shapefile format by
  grouping consecutive points into MultiPointZ records. The default
  size is 1024. It can be changed with '-record 2048'. If you want
  to use PointZ records instead you need to add '-single_points' to
  the command line
 
  Please license from martin.isenburg@rapidlasso.com to use las2shp
  commercially.

  For updates check the website or join the LAStools mailing list.

  http://lastools.org/
  http://groups.google.com/group/lastools/
  http://twitter.com/lastools/
  http://facebook.com/lastools/
  http://linkedin.com/groups?gid=4408378

  Martin @lastools

****************************************************************

example usage:

>> las2shp -i *.las

converts all LAS files matching '*.las' to ESRI's Shapefile format
'*.shp' using MultiPointZ records containing 1024 points each.

>> las2shp -i lidar.laz -o shapefile.shp -record 2048

converts the LAZ file 'lidar.las' to ESRI's Shapefile 'shapefile.shp'
using MultiPointZ records containing 2048 points each.

>> las2shp -lof file_list.txt -merged -o lidar.shp -record 2048

converts the contents of all LAS files listed in 'file_list.txt' to ESRI's
Shapefile format 'lidar.shp' using MultiPointZ records containing 2048
points each.

for more info:

D:\lastools\bin>las2shp -h
Filter points based on their coordinates.
  -keep_tile 631000 4834000 1000 (ll_x ll_y size)
  -keep_circle 630250.00 4834750.00 100 (x y radius)
  -keep_xy 630000 4834000 631000 4836000 (min_x min_y max_x max_y)
  -drop_xy 630000 4834000 631000 4836000 (min_x min_y max_x max_y)
  -keep_x 631500.50 631501.00 (min_x max_x)
  -drop_x 631500.50 631501.00 (min_x max_x)
  -drop_x_below 630000.50 (min_x)
  -drop_x_above 630500.50 (max_x)
  -keep_y 4834500.25 4834550.25 (min_y max_y)
  -drop_y 4834500.25 4834550.25 (min_y max_y)
  -drop_y_below 4834500.25 (min_y)
  -drop_y_above 4836000.75 (max_y)
  -keep_z 11.125 130.725 (min_z max_z)
  -drop_z 11.125 130.725 (min_z max_z)
  -drop_z_below 11.125 (min_z)
  -drop_z_above 130.725 (max_z)
  -keep_xyz 620000 4830000 100 621000 4831000 200 (min_x min_y min_z max_x max_y max_z)
  -drop_xyz 620000 4830000 100 621000 4831000 200 (min_x min_y min_z max_x max_y max_z)
Filter points based on their return number.
  -first_only -keep_first -drop_first
  -last_only -keep_last -drop_last
  -keep_middle -drop_middle
  -keep_return 1 2 3
  -drop_return 3 4
  -keep_single -drop_single
  -keep_double -drop_double
  -keep_triple -drop_triple
  -keep_quadruple -drop_quadruple
  -keep_quintuple -drop_quintuple
Filter points based on the scanline flags.
  -drop_scan_direction 0
  -scan_direction_change_only
  -edge_of_flight_line_only
Filter points based on their intensity.
  -keep_intensity 20 380
  -drop_intensity_below 20
  -drop_intensity_above 380
  -drop_intensity_between 4000 5000
Filter points based on their classification.
  -keep_class 1 3 7
  -drop_class 4 2
  -drop_synthetic -keep_synthetic
  -drop_keypoint -keep_keypoint
  -drop_withheld -keep_withheld
Filter points based on their user data.
  -keep_user_data 1
  -drop_user_data 255
  -keep_user_data_between 10 20
  -drop_user_data_below 1
  -drop_user_data_above 100
  -drop_user_data_between 10 40
Filter points based on their point source ID.
  -keep_point_source 3
  -keep_point_source_between 2 6
  -drop_point_source 27
  -drop_point_source_below 6
  -drop_point_source_above 15
  -drop_point_source_between 17 21
Filter points based on their scan angle.
  -keep_scan_angle -15 15
  -drop_abs_scan_angle_above 15
  -drop_scan_angle_below -15
  -drop_scan_angle_above 15
  -drop_scan_angle_between -25 -23
Filter points based on their gps time.
  -keep_gps_time 11.125 130.725
  -drop_gps_time_below 11.125
  -drop_gps_time_above 130.725
  -drop_gps_time_between 22.0 48.0
Filter points based on their wavepacket.
  -keep_wavepacket 0
  -drop_wavepacket 3
Filter points with simple thinning.
  -keep_every_nth 2
  -keep_random_fraction 0.1
  -thin_with_grid 1.0
Transform coordinates.
  -translate_x -2.5
  -scale_z 0.3048
  -rotate_xy 15.0 620000 4100000 (angle + origin)
  -translate_xyz 0.5 0.5 0
  -translate_then_scale_y -0.5 1.001
  -clamp_z_below 70.5
  -clamp_z 70.5 72.5
Transform raw xyz integers.
  -translate_raw_z 20
  -translate_raw_xyz 1 1 0
  -clamp_raw_z 500 800
Transform intensity.
  -scale_intensity 2.5
  -translate_intensity 50
  -translate_then_scale_intensity 0.5 3.1
  -clamp_intensity 0 255
  -clamp_intensity_above 255
Transform scan_angle.
  -scale_scan_angle 1.944445
  -translate_scan_angle -5
  -translate_then_scale_scan_angle -0.5 2.1
Change the return number or return count of points.
  -repair_zero_returns
  -set_return_number 1
  -change_return_number_from_to 2 1
  -set_number_of_returns 2
  -change_number_of_returns_from_to 0 2
Modify the classification.
  -set_classification 2
  -change_classification_from_to 2 4
  -classify_z_below_as -5.0 7
  -classify_z_above_as 70.0 7
  -classify_z_between_as 2.0 5.0 4
  -classify_intensity_above_as 200 9
  -classify_intensity_below_as 30 11
Modify the user data.
  -set_user_data 0
  -change_user_data_from_to 23 26
Modify the point source ID.
  -set_point_source 500
  -change_point_source_from_to 1023 1024
  -quantize_Z_into_point_source 200
Transform gps_time.
  -translate_gps_time 40.50
  -adjusted_to_week
  -week_to_adjusted 1671
Transform RGB colors.
  -scale_rgb_down (by 256)
  -scale_rgb_up (by 256)
Supported LAS Inputs
  -i lidar.las
  -i lidar.laz
  -i lidar1.las lidar2.las lidar3.las -merged
  -i *.las - merged
  -i flight0??.laz flight1??.laz
  -i terrasolid.bin
  -i esri.shp
  -i nasa.qi
  -i lidar.txt -iparse xyzti -iskip 2 (on-the-fly from ASCII)
  -i lidar.txt -iparse xyzi -itranslate_intensity 1024
  -lof file_list.txt
  -stdin (pipe from stdin)
  -rescale 0.01 0.01 0.001
  -rescale_xy 0.01 0.01
  -rescale_z 0.01
  -reoffset 600000 4000000 0
Supported LAS Outputs
  -o lidar.las
  -o lidar.laz
  -o xyzta.txt -oparse xyzta (on-the-fly to ASCII)
  -o terrasolid.bin
  -o nasa.qi
  -odir C:\data\ground (specify output directory)
  -odix _classified (specify file name appendix)
  -ocut 2 (cut the last two characters from name)
  -olas -olaz -otxt -obin -oqfit (specify format)
  -stdout (pipe to stdout)
  -nil    (pipe to NULL)
LAStools (by martin@rapidlasso.com) version 140301 (unlicensed)
usage:
las2shp -i *.las
las2shp -i *.txt -iparse xyza -keep_scan_angle -10 10
las2shp -i lidar.las -o shapefile.shp -record_size 2048
las2shp -i lidar.laz -last_only -record_size 10000
las2shp -i lidar.laz -keep_class 2 8
las2shp -i *.laz -drop_return 1
las2shp -h

---------------

if you find bugs let me (martin.isenburg@rapidlasso.com) know.
