<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.28.11-Firenze">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["S-JTSK / Krovak East North",BASEGEOGCRS["S-JTSK",DATUM["System of the Unified Trigonometrical Cadastral Network",ELLIPSOID["Bessel 1841",6377397.155,299.1528128,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4156]],CONVERSION["Krovak East North (Greenwich)",METHOD["Krovak (North Orientated)",ID["EPSG",1041]],PARAMETER["Latitude of projection centre",49.5,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8811]],PARAMETER["Longitude of origin",24.8333333333333,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8833]],PARAMETER["Co-latitude of cone axis",30.2881397527778,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",1036]],PARAMETER["Latitude of pseudo standard parallel",78.5,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8818]],PARAMETER["Scale factor on pseudo standard parallel",0.9999,SCALEUNIT["unity",1],ID["EPSG",8819]],PARAMETER["False easting",0,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["GIS."],AREA["Czechia; Slovakia."],BBOX[47.73,12.09,51.06,22.56]],ID["EPSG",5514]]</wkt>
      <proj4>+proj=krovak +lat_0=49.5 +lon_0=24.8333333333333 +alpha=30.2881397527778 +k=0.9999 +x_0=0 +y_0=0 +ellps=bessel +towgs84=589,76,480,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>26812</srsid>
      <srid>5514</srid>
      <authid>EPSG:5514</authid>
      <description>S-JTSK / Krovak East North</description>
      <projectionacronym>krovak</projectionacronym>
      <ellipsoidacronym>EPSG:7004</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
